**HO CHI MINH CITY UNIVERSITY OF TECHNOLOGY**

**VIETNAM NATIONAL UNIVERSITY HO CHI MINH CITY**

🙞∙∙∙☼∙∙∙🙜



**PROJECT**

**(TR4091)**

**DESIGN A MEASURING SYSTEM AND METHOD FOR MEASURING THE SPEED OF AN ALTERNATOR**

**Semester: 241**

Under the guidance of: Ph.D Trần Đăng Long

Student in charge: Nguyễn Quốc Kiệt

Student’s ID: 1952802

*Ho Chi Minh City – 2025*

**PROJECT ASSIGNMENT**

Student’s full name: Nguyễn Quốc Kiệt Student’s ID: 1952802

**Training program:** Automotive Engineering **Class:** CC20KT0

1. **Project title:** Design of measuring system and method for measuring the speed of an alternator.
2. **Requested content:** The system is designed to accurately measure important parameters including frequency and operating speed of the alternator.

* Measurement: error less than 5%
* Measuring range:
* Graphical user interface: clear and user-friendly

1. **Requested products:**

◻ Full report ◻ Poster ◻ Scientific paper



◻ Software ◻ Firmware ◻ Numerical model

◻ General layout drawings ◻ Detailed drawings ◻ Assembly drawings

◻ Others: Simulation on Proteus

1. **Date of assignment:**  10/10/2024
2. **Date of accomplishment:** 29/12/2024

**The project assignment is approved by the Department of Automotive Engineering.**

|  |  |
| --- | --- |
| *Date:* 02/01/2025  **Head of Department** | *Date:* 02/01/2025  **Project Advisor** |

**ABSTRACT**

This project presents the design and development of an on-board alternator speed measurement system. The system is designed to accurately measure critical parameters including frequency and speed. The focus is placed on the programming aspect to optimize the algorithms for accurate measurement and low error control.

The study delves into the intricacies of programming techniques and algorithm optimization to ensure high accuracy in measurement and minimal error in control processes. Through meticulous design and implementation, the developed system proves its effectiveness in providing reliable and accurate data, which is crucial for engine speed performance analysis. Furthermore, the potential applications of the system have grown beyond the scope of the current study.

This project lays the foundation for further advances in the field of embedded systems that promise significant contributions to the field of sustainable transport.

# TABLE OF CONTENT

[ABSTRACT 1](#_Toc189581921)

[TABLE OF CONTENT 2](#_Toc189581922)

[LIST OF TABLE 4](#_Toc189581923)

[LIST OF FIGURE 5](#_Toc189581924)

[1. INTRODUCTION 7](#_Toc189581925)

[1.1. Project’s type: 7](#_Toc189581926)

[1.2. Project’s main object: 7](#_Toc189581927)

[1.3. Project’s targets: 7](#_Toc189581928)

[1.4. Operating conditions: 7](#_Toc189581929)

[1.5. Technical requirements: 7](#_Toc189581930)

[1.6. Proposed solution: 8](#_Toc189581931)

[1.7. Task to be done: 9](#_Toc189581932)

[1.8. Scope of project: 10](#_Toc189581933)

[2. THEORETICAL BASIS 11](#_Toc189581934)

[2.1. Alternator 11](#_Toc189581935)

[2.1.1. Rotor 12](#_Toc189581936)

[2.1.2. Rectifier 13](#_Toc189581937)

[2.1.3. Cooling mechanism: 13](#_Toc189581938)

[2.1.4. Housing and Bearing 14](#_Toc189581939)

[2.2. Schmitt trigger: 14](#_Toc189581940)

[2.3. Microcontroller 15](#_Toc189581941)

[2.4. UART communications 16](#_Toc189581942)

[2.4.1. Serial class 17](#_Toc189581943)

[2.4.2. Arduino UART Pins 17](#_Toc189581944)

[2.4.3. Working principle of UART: 18](#_Toc189581945)

[3. GENERAL LAYOUT DESIGN 21](#_Toc189581946)

[4. TECHNICAL DESIGN 23](#_Toc189581947)

[4.1. Voltage divider design 23](#_Toc189581948)

[4.2. Schmitt trigger circuit design 23](#_Toc189581949)

[4.3. Wiring diagram 25](#_Toc189581950)

[4.4. Timing diagram 26](#_Toc189581951)

[4.5. Work flows 28](#_Toc189581952)

[4.6. Algorithms 30](#_Toc189581953)

[5. SIMULATIONS AND RESULTS 32](#_Toc189581954)

[5.1. Const frequency case: 32](#_Toc189581955)

[5.2. Real-time frequency case: 36](#_Toc189581956)

[6. CONCLUSION: 39](#_Toc189581957)

[7. REFERENCE 40](#_Toc189581958)

# LIST OF TABLE

[Table 1: Arduino Uno board pin 18](#_Toc187690530)

[Table 2. Results for the fixed frequency case show errors 35](#_Toc187690531)

[Table 3. Results for the real-time frequency case show errors 37](#_Toc187690532)

# LIST OF FIGURE

[Figure 1. V-Model 9](#_Toc189582666)

[Figure 2. Construction of an alternator 11](#_Toc189582667)

[Figure 3. Alternator rotor 12](#_Toc189582668)

[Figure 4. Alternator Rectifier 13](#_Toc189582669)

[Figure 5. Alternator cooling mechanism 13](#_Toc189582670)

[Figure 6. Non-symmetrical Schmitt Trigger using OP-Amp with single power 14](#_Toc189582671)

[Figure 7. Transfer function of a Schmitt trigger 15](#_Toc189582672)

[Figure 8. Arduino Uno Microcontroller Board 16](#_Toc189582673)

[Figure 9. Serial / parallel communication 18](#_Toc189582674)

[Figure 10. Start bit 19](#_Toc189582675)

[Figure 11. Data bit 20](#_Toc189582676)

[Figure 12. Parity bit 20](#_Toc189582677)

[Figure 13. Stop bit 21](#_Toc189582678)

[Figure 14. General layout diagram 22](#_Toc189582679)

[Figure 15. Schmitt trigger input and output waveform 24](#_Toc189582680)

[Figure 16. Wiring diagram of measuring system the speed of an alternator 25](#_Toc189582681)

[Figure 17. Timing diagram 26](#_Toc189582682)

[Figure 18. Work-flows 28](#_Toc189582683)

[Figure 19. Algorithms 30](#_Toc189582684)

[Figure 20. Program simulation on Proteus 32](#_Toc189582685)

[Figure 21. Results in const frequency case 33](#_Toc189582686)

[Figure 25. Code in Timer Interrupt 34](#_Toc189582687)

[Figure 22. Program simulation on Proteus 35](#_Toc189582688)

[Figure 23.. Program simulation on Proteus 36](#_Toc189582689)

[Figure 24. Results in real-time frequency case 37](#_Toc189582690)

1. **INTRODUCTION**
   1. **Project’s type:**

Design an embedded system for automotive applications.

* 1. **Project’s main object:**

The objective of the project is to design a system to measure the speed of the generator on a vehicle by combining hardware and software. The system will measure, calculate and display the rotation speed of an alternator.

* 1. **Project’s targets:**

Design a measuring system and method for measuring the speed of an alternator based on the one phase voltage of an alternator.

* 1. **Operating conditions:**

- The alternator is removed from the vehicle and driven by an external motor for controlled testing.

- The alternator is in optimal working condition, ensuring accurate measurement results.

- The alternator operates under no-load conditions, eliminating the influence of external electrical loads.

- The microcontroller operates for a short duration, approximately 30 minutes per test session.

- All electrical components are in excellent condition, carefully inspected, and tested prior to operation to ensure reliability.

* 1. **Technical requirements:**

**Functions:**

- Measure the speed of an alternator continously and in real-time.

**-** Speed range from 500 to 15000 RPM

- Display clear, user-friendly graphical user interface for monitoring.

- Display sufficient parameters for monitoring.

- Provide clear, sizable screen with appropriate notation.

**Techniques:**

- The ambient room temperature is maintained at 30°C under stable conditions, with no external shock or vibrations affecting the system.

- Use an LCD screen via UART communication to display the falling edge moment, frequency, overflow count, and measured speed of an alternator.

**Efficiencies and Durability:**

**-** Measured parameters frequency and speed of an alternator have an error is less than 1%.

- Compact size, suitable for automotive installation.

- Power-efficient design.

- Low maintenance cost, robust operation in automotive environments.

* 1. **Proposed solution:**

The alternator's output frequency is directly related to the rotor speed and the number of pole pairs.

By measuring the frequency of the alternator’s output voltage, the system can determine the rotational speed.

The output signals which is generated by the alternator are the sine wave form, while, the microcontroller is only capable of reading the digital signals. A signal conditioning circuit must be used to convert the alternator’s AC voltage into a square wave signal suitable for microcontroller processing. (main hardware design).

The Arduino reads the frequency, calculates the speed, and displays it on an LCD screen. (main software design).

* 1. **Task to be done:**

**A diagram of software testing

Description automatically generated**

Figure 1. V-Model

The V-diagram in the figure depicts the embedded system development process according to the V-Model, in which the development phase (left) is reflected by the corresponding testing phases (right).

* **Objectives & Technical requirements: (Section 1 – Introduction)**

This is the stage where you define what the system should do. This could include functional requirements (what tasks the system should perform) and non-functional requirements (constraints like cost and size).

* **System design: (Section 3*-4* – General layout design)**

*Hardware*: Arduino, signal conditioning circuit, LCD screen, UART communication.

*Software*: Frequency measurement, speed calculation, real-time display.

* **Subsystem design: (Section 4 – Technical design)**

*Hardware design:*

- Schematic diagram and circuit.

- Connection between Arduino, signal conditioning circuit, LCD, UART.

- Select appropriate components to ensure accuracy and stability.

Software design: Timing diagrams,work-flows, algorithms, error handling.

* **Testing: (Section 5 – Simulations and Results)**

*Unit Testing:*

- Testing individual modules

- Is the pulse signal reading correct?

- Is the speed calculation correct?

- Is the LCD/UART display working?

*Integration Testing:*

- Testing the software when combined with the hardware. Ensuring the measurement and display data are correct.

*System Testing:*

- Testing the entire system in simulation and in real life. Measuring the speed with a real transmitter, comparing it to a standard device.

*Acceptance Testing:*

- Comparing the actual results with the original requirements.

- Evaluating the accuracy, performance, and durability of the system.

* 1. **Scope of project:**

- Designing a generator speed measurement simulation interface using Proteus.

- Enhance the user interface, either through an LCD touchscreen or mobile app.

1. **THEORETICAL BASIS**
   1. **Alternator**

The alternator is the part that generates and supplies electrical energy to the battery and other electrical systems on the vehicle when the engine is running. The alternator is driven by a belt connected to the crankshaft pulley, converting mechanical energy into electrical energy.

The alternator is usually located in the engine compartment and is designed to provide electrical energy to other systems immediately after the engine is running, while also recharging the auxiliary battery.




Figure 2. Construction of an alternator

* + 1. **Rotor**

The rotor plays a crucial role in producing the rotating magnetic field required for electricity generation.




Figure 3. Alternator rotor

It is composed of main components:

Field Winding: This is a coil wrapped around an iron core that, when energized with a small current, generates a magnetic field.

Slip Rings and Brushes: These elements deliver current to the rotor, enabling it to rotate while maintaining an electrical connection.

Pawl Poles: These are projections that strengthen the magnetic field, alternating between north and south poles.

As the rotor rotates, its magnetic field intersects with the stator windings, inducing an alternating current (AC).

* + 1. **Rectifier**




Figure 4. Alternator Rectifier

The rectifier is an essential part of the system, responsible for converting the alternating current (AC) generated by the stator into direct current (DC). This DC output is crucial for charging the battery and operating the vehicle's electrical components. It generally includes six diodes configured in a bridge arrangement to provide a stable DC output.

* + 1. **Cooling mechanism:**

**Diagram of a car engine

Description automatically generated**

Figure 5. Alternator cooling mechanism

Since alternators generate a significant amount of heat during operation, an efficient cooling system is essential. Modern alternators use internal fans or external cooling fins to dissipate heat and maintain optimal operating temperatures.

* + 1. **Housing and Bearing**

The alternator’s end covers protect its internal components and provide structural support. Bearings located at either end of the rotor shaft allow for smooth rotation and reduce friction, enhancing the alternator’s efficiency and lifespan.

* 1. **Schmitt trigger:**

Hysteresis: This is the defining feature of Schmitt Trigger. This means that the output voltage depends on the previous values of the input signal. This hysteresis helps in creating two different voltage thresholds. The first threshold value is for the rising input and the other is for the falling input signal a basic

A diagram of a circuit

Description automatically generated

Figure 6. Non-symmetrical Schmitt Trigger using OP-Amp with single power

Noise rejection: Hysteresis helps in eliminating noise. When there are small fluctuations in the input signal, the output signal does not change or show false values. It helps in preventing noise from the noisy environment.

The circuit is named a trigger because the output retains its value until the input changes sufficiently to trigger a change. In the non-inverting configuration, when the input is higher than a chosen threshold, the output is high. When the input is below a different (lower) chosen threshold the output is low, and when the input is between the two levels the output retains its value. This dual threshold action is called hysteresis and implies that the Schmitt trigger possesses memory and can act as a bistable multivibrator (latch or flip-flop). There is a close relation between the two kinds of circuits: a Schmitt trigger can be converted into a latch and a latch can be converted into a Schmitt trigger.

In this circuit, the two resistors R1 and R2 form a parallel voltage summer. It adds a part of the output voltage to the input voltage thus augmenting it during and after switching that occurs when the resulting voltage is near ground. This parallel positive feedback creates the needed hysteresis that is controlled by the proportion between the resistances of R1 and R2. The output of the parallel voltage summer is single-ended (it produces voltage with respect to ground) so the circuit does not need an amplifier with a differential input. Since conventional op-amps have a differential input, the inverting input is grounded to make the reference point zero volts.

A diagram of a square with red lines and blue arrows

Description automatically generated

Figure 7. Transfer function of a Schmitt trigger

The horizontal and vertical axes are input voltage and output voltage, respectively. T and −T are the switching thresholds, and M and −M are the output voltage levels.

* 1. **Microcontroller**

To read the voltage signal of the generator, we need to use a microprocessor, we use the Arduino board. Arduino is an open source platform based on the C/C++ programming language. Arduino includes a computer programming software and hardware versions of Arduino boards serving a variety of purposes.

Arduino Uno R3 is an open source microcontroller board based on the Microchip ATmega328 microcontroller developed by Arduino.cc. The board is equipped with Digital and Analog input/output pins that can interface with various expansion boards.

A blue electronic board with black wires

Description automatically generated

Figure 8. Arduino Uno Microcontroller Board

The Arduino Uno R3 board provides us with:

* 20 digital input/output pins, of which 7 can provide pulse width modulation (PWM) output signals: 3, 5, 6, 9, 10, 11, and 13.
* 6 analog input pins: A0 🡪 A5. Pins A0 🡪 A5 are located in the same position as the Arduino Leonardo board. Each pin has a 10-bit resolution. All of these pins can be used as digital I/O pins.
* 3 Timers/Counters: TIMER0, TIMER1, TIMER2 support fixed-periodic operation of some functions.
* An 8-bit microprocessor chip operating at 16MHz.

Using the Arduino board, within the framework of this project, the following tasks will be performed: reading the generator voltage signal values, overflow values, values ​​at the time of falling edge triggering and calculating the generator frequency and speed.

* 1. **UART communications**

Universal Asynchronous Receiver-Transmitter (UART), a serial communication protocol that can be used to send data between an Arduino board and other devices. This is the protocol used when you send data from an Arduino to your computer, using the classic Serial.print() method.

UART is one of the most used device-to-device (serial) communication protocols. It’s the protocol used by Arduino boards to communicate with the computer. It allows an asynchronous serial communication in which the data format and transmission speed are configurable. It's among the earliest serial protocols and even though it has in many places been replaced by SPI and I2C it's still widely used for lower-speed and lower-throughput applications because it is very simple, low-cost and easy to implement.

Communication via UART is enabled by the Serial class, which has a number of methods available, including reading & writing data.

* + 1. **Serial class**

With the Serial class, you can send / receive data to and from your computer over USB, or to a device connected via the Arduino's RX/TX pins.

* When sending data over USB, we use Serial. This data can be viewed in the Serial Monitor in the Arduino IDE.
* When sending data over RX/TX pins, we use Serial1.
* The GIGA R1 WiFi, Mega 2560 and Due boards also have Serial2 and Serial3
* The Serial class have several methods with some of the essentials being:

+ begin() - begins serial communication, with a specified baud rate (many examples use either 9600 or 115200).

+ print() - prints the content to the Serial Monitor.

+ println() - prints the content to the Serial Monitor, and adds a new line.

+ available() - checks if serial data is available (if you send a command from the Serial Monitor).

+ read() - reads data from the serial port.

+ write() - writes data to the serial port.

* + 1. **Arduino UART Pins**

The default TX/RX pins on an Arduino board are the D0(RX) and D1(TX) pins. Some boards have additional serial ports, see table below:

| **Form Factor** | **RX** | **TX** | **RX1** | **TX1** | **RX2** | **TX2** | **RX3** | **TX3** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| MKR | D0 | D1 |  |  |  |  |  |  |
| UNO | D0 | D1 |  |  |  |  |  |  |
| Nano | D0 | D1 |  |  |  |  |  |  |
| Mega | D0 | D1 | D19 | D18 | D17 | D16 | D15 | D14 |

Table 1: Arduino Uno board pin

* + 1. **Working principle of UART:**

UART operates by transmitting data as a series of bits, including a start bit, data bits, an optional parity bit, and stop bit(s). Unlike parallel communication, where multiple bits are transmitted simultaneously, UART sends data serially, one bit at a time. As the name reveals the protocol operates asynchronous which means that it doesn't rely on a shared clock signal. Instead, it uses predefined baud rates to determine the timing of data bits.

A diagram of a parallel communication

Description automatically generated

Figure 9. Serial / parallel communication

**Start Bit:**

A single start bit is transmitted at the beginning of each UART frame. The primary purpose of the start bit is to indicate the start of the data transmission and prepare the receiver for data reception.

The start bit is always logic low (0) for UART communication. This means that the start bit is transmitted as a voltage level that is lower than the logic high threshold, typically at the receiver's end.

When the receiver detects a start bit, it knows that a new data frame is beginning, and it prepares to receive the incoming bits.

A screenshot of a video game

Description automatically generated

Figure 10. Start bit

**Data bits:**

Data bits are a fundamental component of UART communication as they carry the actual information to be transmitted. The number of data bits in a UART frame can vary, but a common and widely used configuration is 8 bits. However, UART supports various character sizes, including 7-bit and 6-bit configurations, depending on the specific application requirements.

A screen shot of a computer

Description automatically generated

Figure 11. Data bit

**Parity bits:**

In addition to data bits, UART communication may include a parity bit as part of the data frame. Parity is an error-checking mechanism that can help detect data transmission errors. Parity can be set to "odd" or "even," and it ensures that the total number of bits set to logic "1" in a character is either even or odd, depending on the chosen parity type. The presence of a parity bit allows the receiver to verify the integrity of the received data. If the number of "1" bits don't match the expected parity, an error is detected.

A graphic of a diagram

Description automatically generated with medium confidence

Figure 12. Parity bit

**Stop bits:**

One or more stop bits are sent after the data bits within each UART frame. The stop bit(s) signal the end of the data byte and serve to indicate the conclusion of data transmission. The most common configuration is to use one stop bit, but in situations where added reliability is required, two stop bits can be employed.

A screenshot of a computer

Description automatically generated

Figure 13. Stop bit

1. **GENERAL LAYOUT DESIGN**

After identifying the main components of the system, we divide the main components into functional clusters that undertake specific tasks.

To solve the problem in the topic, the generator speed measurement system is determined to include four functional clusters:

- Signal generation cluster

- Signal conditioning cluster

- Signal reading and frequency calculation cluster

- Display cluster

With the functional clusters arranged, we also need to determine the path of the signals and the interactions between the functional clusters.

In this section, we will solve the issues: General layout diagram.

A diagram of a computer system

Description automatically generated

Figure 14. General layout diagram

* **Signal generation cluster:**
* Generates a 3-phase AC voltage signal when the rotor rotates.
* Output signal: AC (Analog) sine wave, containing information about the frequency (f), depending on the rotor rotation speed
* **Signal conditioning cluster:**
* Using a voltage divider circuit to match the input voltage level of the Arduino (0–5V).
* Convert the AC signal from the generator into a digital signal that the microcontroller can read.
* Use a Schmitt Trigger circuit to convert the sine wave signal into a square wave**.**
* **Signal reading and frequency calculation cluster:**
* Input signal: Square pulse signal (Digital Signal) from the signal conditioning block.
* Use Timer1 to measure the number of values ​​that the Timer/Counter 1 has counted between two falling edges of the pulse.
* Calculate the rotational speed (RPM) based on the formula:
* Output signal: Speed, T1, T2, Overf, f data as Serial Data.
* Transmit to: Display Block
* **Display cluster:**
* Input signal: Processed data from Microcontroller.
* Display measured parameters including: Speed, Frequency, Overflow, T1, T2
* Help users observe and evaluate measurement results.

1. **TECHNICAL DESIGN**
   1. **Voltage divider design**

Because the Arduino UNO R3 maximum input voltage is 5V, so we have to use it in order to reduce the phase voltage, from nearly 14V to this value

* **Calculation:**

Choose

Apply the formula for calculating **:**

* 1. **Schmitt trigger circuit design**

The output signals which is generated by the alternator are the sine wave form. However, the microcontroller is only capable of reading the digital signals, so that we have to convert the input signal to digital signal by using this circuit.

A diagram of a voltage

Description automatically generated

Figure 15. Schmitt trigger input and output waveform

When , the voltage across becomes the Upper Threshold Voltage (). The input voltage, , must be slightly more positive than to cause the output to switch from to . When the input voltage is less than , the output voltage is at .

**Upper Threshold Voltage:** = + ( / [ + ])

When , the voltage across is called the Lower Threshold Voltage (). The input voltage, , must be slightly more negative than to cause the output to switch from to . When the input voltage is less than , the output voltage is at .

**Lower Threshold Voltage:** = ( / [ + ])

* **Calculation:**

Choose ; ;

Choose ;

Calculate the high and low threshold.

* High threshold:
* Low threshold:
  1. **Wiring diagram**

**A diagram of a circuit board

Description automatically generated**

Figure 16. Wiring diagram of measuring system the speed of an alternator

First, the generator operates and generates a signal in the form of a sine wave, with an operating voltage of about 14V. Since the microcontroller only receives signals from 0 to 5V, this signal is passed through a signal processing circuit to convert the voltage from 14 to 5V. Here, I have passed it through a voltage regulator with two resistors of 10 ohms and 5.5 ohms respectively.

Since the generator signal is a sine wave, we need to process this signal into a square wave to suit the microcontroller. We will pass it through a schmitt trigger circuit to convert the signal from a sine wave to a square wave with an amplitude ranging from 0V to 5V.

Then, the microprocessor will read the signal and calculate the frequency, speed of this square wave and then send the value it reads to the screen for the user.

* 1. **Timing diagram**

**A diagram of a graph

Description automatically generated**

Figure 17. Timing diagram

The timing diagram describes the counting process of the Timer/Counter1 counter.

Where:

: the period of Alternator signal.

the frequency of Alternator signal

TOP: the peak value at which the Timer/Counter1 changes state.

BOTTOM: the lowest value that a Timer/Counter 1 reaches.

: count value of Timer/Counter1 that counted from to .

n: number of overflow.

at the falling edge of the speed signal.

at the next falling edge of the speed signal

: count value of Timer/Counter 1 at .

: count value of Timer/Counter1 at .

From the timing diagram above, we can calculate as follows:

Count value of Timer/Counter1:

Frequency of alternator:

Rotational speed of alternator:

Where:

:count value of Timer/Counter1 that counted from to .

: the period of Alternator signal.

the frequency of Alternator signal

clock speed of Arduino ( )

Prescaler: frequency divider (= 64)

the frequency of Timer/Counter 1.

S: Rotational speed of an alternator

P: number of pair poles

* 1. **Work flows**

**A diagram of a computer program

Description automatically generated**

Figure 18. Work-flows

❖ **Priority and workload of each task when implementing the program:**

**Fixed periodic repetition work:**

* Check flag status
* Check if data from Timer is complete
* Display calculated data on screen

**Random repetitive work:**

* At : Jump to interrupt program of the falling edge: and set .
* After, exit interrupt program and the program continues execution. Until Timer/Counter1 overflow, jump to interrupt program Overflow and n++

( if n > 1 🡪 n =0 )

* At : Jump to interrupt program of the next falling edge:

and after that, save , then save value into global variables.

calculate the value of: 🡪 Calculate f 🡪 Calculate S 🡪 Serial display (Delay 1000ms).

Reset: When: n != 0 🡪 , n = 0

n = 0 🡪 (ko update)

* Continues program, at : Save ; . Save .

Then, calculate:

Reset: When n != 0 🡪 , n = 0

n = 0 🡪 (ko update)

* **Advantage of work-flows:**

Workflow organization: Helps programmers and development teams understand the steps involved in a software project from start to finish. This includes planning, coding, testing, and deployment.

Increase productivity: A clear workflow helps avoid unnecessary repetition, reduces errors, and speeds up project completion.

Quality assurance: Workflows often include quality checks such as code review, automated testing, and continuous integration testing, ensuring that the source code meets certain standards.

Workflow assignment: For team projects, workflows help to properly divide work among members, define responsibilities, and track progress.

Version control: Workflows are often integrated with version control tools such as Git to track source code changes and handle conflicts when multiple people work on the same project.

Easy to extend and maintain: Clear workflows make it easier to extend and maintain the software, as the steps are standardized and documented.

Better collaboration: Workflows support effective communication between team members, reducing misunderstandings and enhancing coordination.

* 1. **Algorithms**

A diagram of a computer program

Description automatically generated with medium confidence

Figure 19. Algorithms

First is main program initialization

**Setup function: (Void setup)**

System initialization.

Timer1 configuration

Reset all register

Set prescaler

Enable input capture interrupt

Enable overflow interrupt

**Interrupt function**.

ISR: TIMER1\_CAPT\_vect

Activated automatically and occurs when there is a falling edge interrupt of the input signal.

Recording the time of the falling edge interrupt, it will record the value of , .

ISR: TIMER1\_OVF\_vect

Activated automatically and occurs when the Timer1 counter overflows, that is, when counting to 65535.

**Loop function: (Void loop)**

Check if there are enough triples of numbers , and n to calculate the speed

Check the signal flag to display the value on the screen

Reset the variables to serve the calculation for the next cycle.

The function executes continuously throughout the system.

1. **SIMULATIONS AND RESULTS**
   1. **Const frequency case:**

A computer screen shot of a circuit board

Description automatically generated

Figure 20. Program simulation on Proteus

Using the Proteus Software to simulate. In real life, alternator’s RPM and frequency vary depending on the engine load. However, 3- phase generator model in Proteus just can run at a constant frequency, so it is hard to prove that our design running smoothly in practice.

A screenshot of a computer

Description automatically generated

A screenshot of a computer screen

Description automatically generated

Figure 21. Results in const frequency case

**Check timer overflow cycle:**

The simplest way is to print the overflow count every second to observe and check whether the displayed overflow count is correct with the analyzed result.

Cycle of Timer/Counter1:

Time for Timer/Counter1 to count from 0 to 65535:

But the time we need to create is 0.01s so that overflow.

Therefore, we need counts. Initial value of TCNT1 = 65536 - 2500 = 63035.

A computer screen shot of a code

Description automatically generated

Figure 25. Code in Timer Interrupt

Here, I have set the Timer to overflow after 10ms, which means that after 1s it will overflow 100 times.

For example, overflow count displayed on Virtual Terminal:

after 2 seconds 🡪 

Conclusion: timer operates with correct required overflow cycle.

**Add one task:**

In the program, I have added 1 task to check if the program runs stably or not.

Every time an overflow interrupt occurs, I will control the activation of pin D7 (Digital Output), if it is at level 1 then it will go down to level 0 and opposite.

If it happens as the above condition, then the program I organized is correct.

A screen shot of a graph

Description automatically generated

Figure 22. Program simulation on Proteus

Conclusion: The program run correct as requested.

**Check the results:**

F: Input Frequency (Hz).

(RPM), P = 3: number of pole pairs

: measured frequency in fixed case

(RPM)

: error when measuring in fixed case

A screenshot of a screen

Description automatically generated

Table 2. Results for the fixed frequency case show errors

The fixed frequency case: in this case, we will stop the simulation and change the fixed frequency to test whether our code run well.

* 1. **Real-time frequency case:**

In this case, we will use an activepotentiometer in Proteus to simulate the variation of frequency by changing the input voltage. The ADC function of Arduino will read and calculate the input voltage, then using that value to create a square wave by Arduino CTC mode for Timer1. Then we will recalculate our wave’s frequency to test if the code is fit for practical or not.

A computer circuit board with wires

Description automatically generated with medium confidence

Figure 23.. Program simulation on Proteus

A screenshot of a computer

Description automatically generated

A screenshot of a computer screen

Description automatically generated

Figure 24. Results in real-time frequency case

**Check the results:**

A screenshot of a screen

Description automatically generated

Table 3. Results for the real-time frequency case show errors

* **Evaluation and discussion:**

- The speed measurement system has been functioning accurately within the range of 500 - 15,000 RPM, with an error is less than 1%.

- The system has a 100ms update rate, ensuring real-time measurement.

- The LCD/UART display interface is user-friendly and easy to read.

- The system operates reliably in temperatures between 28-32°C without significant impact. Although there is some noise in the input signal from the alternator, it has been effectively filtered.

- The system has successfully met all functional requirements and the accuracy and performance meet the original specifications.

In conclusion, the project has achieved its targets with high accuracy and has fully met all technical requirements. However, there is room for improvement in optimizing the system, particularly in handling signal noise.

1. **CONCLUSION:**

Based on the results obtained, it can be concluded that our design successfully meets the required technical criteria and functional objectives. The system accurately measures the alternator's speed in real-time, with a measurement range of 500 to 15,000 RPM and an error rate of less than 1%, aligning with our initial project targets.

**Project achievements:** We have successfully designed and implemented an embedded system for automotive applications. Our system achieves real-time speed measurement and displays results on an LCD via UART.

**Future developments:** While our design meets the functional and technical requirements, there are still areas that can be further optimized. These include enhancing noise filtering algorithms to improve measurement precision, expanding the system to integrate with OBD-II for higher accuracy, and developing a mobile interface for real-time monitoring via Bluetooth or Wi-Fi.

1. **REFERENCE**

[1] ATmega48A/PA/88A/PA/168A/PA/328/P **\_** Mega AVR Data Sheet

[2] Trần Đăng Long \_ AEES Material Powerpoint

[3] Wolfgang Ewald (2022), Timer and PWM – Part 2 (16 Bit Timer1), https://wolles-elektronikkiste.de/en/timer-and-pwm-part-2-16-bit-timer1

[4] [Khaled Magdy](https://deepbluembedded.com/author/admin/) (2020), Arduino Counter Timer Mode Tutorial & Code Examples, https://deepbluembedded.com/arduino-counter-timer/